<xml version="Mixly 2.0 rc2" board="Arduino AVR@Arduino/Genuino Uno" xmlns="http://www.w3.org/1999/xhtml"><block type="base_setup" id=",bNEqWc%M~,(5)*xan9j" x="-118" y="61"><statement name="DO"><block type="serial_begin" id="[,DR0*wjZM+RFXuW@G;?"><field name="serial_select">Serial</field><value name="CONTENT"><shadow type="math_number" id="6d]#aL)P665EjKpPVR5:"><field name="NUM">9600</field></shadow></value></block></statement></block><block type="serial_println" id="/0@;XjukIaQT/;`~GV%Y" x="-119" y="149"><field name="serial_select">Serial</field><field name="new_line">println</field><value name="CONTENT"><block type="inout_analog_read" id="J+V;UU{m#KL22_p8Hol*"><value name="PIN"><shadow type="pins_analog" id=".y$j~lZrTijU|0VSDp[T"><field name="PIN">A1</field></shadow></value></block></value><next><block type="base_delay" id="^+2~[d6?C1h[XZvlU!6$"><field name="UNIT">delay</field><value name="DELAY_TIME"><shadow type="math_number" id="F[b]A0/e3ZspHq_JoC%["><field name="NUM">500</field></shadow></value><next><block type="controls_if" id="mE0l3NIMl?@0%m8[7@Pw"><mutation xmlns="http://www.w3.org/1999/xhtml" else="1"></mutation><value name="IF0"><block type="logic_compare" id="TTt3V(c{^9AmDx:^E*!U"><field name="OP">LTE</field><value name="A"><block type="inout_analog_read" id=".4IiW=U#?ea0P(g}+XK~"><value name="PIN"><shadow type="pins_analog" id="$gwx14h5x?vIZuvW|QFQ"><field name="PIN">A1</field></shadow></value></block></value><value name="B"><block type="math_number" id="[k|etTka`}m!Q`h(ib]P"><field name="NUM">400</field></block></value></block></value><statement name="DO0"><block type="inout_digital_write2" id="xT$Pyh#s^ni~n*sh{Ry:"><value name="PIN"><shadow type="pins_digital" id="In/,tzmFrL$7F796D|Wa"><field name="PIN">5</field></shadow></value><value name="STAT"><shadow type="inout_highlow" id="|a7n_FguC6^4)v~z#hSM"><field name="BOOL">HIGH</field></shadow></value><next><block type="base_delay" id="d1vq0L@AdV=WUrC-UI!Y"><field name="UNIT">delay</field><value name="DELAY_TIME"><shadow type="math_number" id="BJ2E9?]vnlM0ee}ftTo."><field name="NUM">500</field></shadow></value></block></next></block></statement><statement name="ELSE"><block type="inout_digital_write2" id="pjeTz/RSk-o-cd022]Yl"><value name="PIN"><shadow type="pins_digital" id="]5kIqKVP33]u97Z(r(l8"><field name="PIN">5</field></shadow></value><value name="STAT"><shadow type="inout_highlow" id="p:EX-67e3Sp?oY]ungkn"><field name="BOOL">LOW</field></shadow></value><next><block type="base_delay" id="-HvCd$XK09;ik9~W0VZ("><field name="UNIT">delay</field><value name="DELAY_TIME"><shadow type="math_number" id="/6g*HAP1PcPEs8=dw/)V"><field name="NUM">500</field></shadow></value></block></next></block></statement></block></next></block></next></block></xml>