<xml version=\"1.2.5\" board=\"Arduino/Genuino Uno\" xmlns=\"http://www.w3.org/1999/xhtml\"><block type=\"base_setup\" id=\"pf$jic}q-l{7NaPmV/1q\" x=\"-12\" y=\"-54\"><statement name=\"DO\"><block type=\"variables_declare\" id=\"NV`gY-Uo*XxQp^M.rSL_\"><field name=\"variables_type\">global_variate</field><field name=\"VAR\">dataPin</field><field name=\"TYPE\">int</field><value name=\"VALUE\"><block type=\"math_number\" id=\"937z=Rj;Hy(Cj_^*/FKv\"><field name=\"NUM\">4</field></block></value><next><block type=\"variables_declare\" id=\"{bM|u[Q7t0Ktcq$AHh~l\"><field name=\"variables_type\">global_variate</field><field name=\"VAR\">clockPin</field><field name=\"TYPE\">int</field><value name=\"VALUE\"><block type=\"math_number\" id=\"h~9Osoeol=WA?KYbK!.l\"><field name=\"NUM\">6</field></block></value><next><block type=\"variables_declare\" id=\"2NjOQhzm{Rb}Sbbr]F^d\"><field name=\"variables_type\">global_variate</field><field name=\"VAR\">latchPin</field><field name=\"TYPE\">int</field><value name=\"VALUE\"><block type=\"math_number\" id=\"uMp+LZ13vC|w8Rc;Yoyl\"><field name=\"NUM\">5</field></block></value></block></next></block></next></block></statement></block><block type=\"controls_for\" id=\"}o}I+26C`n]FN)?d@::l\" x=\"-9\" y=\"80\"><field name=\"VAR\">data</field><value name=\"FROM\"><shadow type=\"math_number\" id=\"C@~hT7xxsu~dr;rjS_$a\"><field name=\"NUM\">0</field></shadow></value><value name=\"TO\"><shadow type=\"math_number\" id=\"ehv(P!Z9*ir5pl-*u(Bw\"><field name=\"NUM\">255</field></shadow></value><value name=\"STEP\"><shadow type=\"math_number\" id=\"{,DE!h5^?3|t;8I/X`wt\"><field name=\"NUM\">1</field></shadow></value><statement name=\"DO\"><block type=\"inout_digital_write2\" id=\"+(7},v+P,}He*2CzbE5V\"><value name=\"PIN\"><shadow type=\"pins_digital\" id=\"nbjLWW8~.1/[FT0}=l`-\"><field name=\"PIN\">0</field></shadow><block type=\"variables_get\" id=\"x~.pk(*t~-Rj^qLF`mTE\"><field name=\"VAR\">latchPin</field></block></value><value name=\"STAT\"><shadow type=\"inout_highlow\" id=\"|djQr=qFG(0Z|nI1kr^a\"><field name=\"BOOL\">LOW</field></shadow></value><next><block type=\"inout_shiftout\" id=\"Nv8i6Fd-zpl0DpZ-v++$\"><field name=\"ORDER\">LSBFIRST</field><value name=\"PIN1\"><shadow type=\"pins_digital\" id=\"+l-ul0Nvl$)JF#WhA2;3\"><field name=\"PIN\">0</field></shadow><block type=\"variables_get\" id=\"{agq?Cm+7[sq8S_!Ku^a\"><field name=\"VAR\">dataPin</field></block></value><value name=\"PIN2\"><shadow type=\"pins_digital\" id=\"_:$FMYoK)4*QnS,~qCYQ\"><field name=\"PIN\">0</field></shadow><block type=\"variables_get\" id=\"inyMH#y3fo{2bdpu!-hV\"><field name=\"VAR\">clockPin</field></block></value><value name=\"DATA\"><shadow type=\"math_number\" id=\"P9QAe$)h[m7LJ:2?#rA5\"><field name=\"NUM\">0</field></shadow><block type=\"variables_get\" id=\"/1??uCyQovSn8.xBF{H.\"><field name=\"VAR\">data</field></block></value><next><block type=\"inout_digital_write2\" id=\"Vum82Mv{q;nh-[dF`^W6\"><value name=\"PIN\"><shadow type=\"pins_digital\" id=\"nbjLWW8~.1/[FT0}=l`-\"><field name=\"PIN\">0</field></shadow><block type=\"variables_get\" id=\"iWV^d~sC#7!B?1ncG1-[\"><field name=\"VAR\">latchPin</field></block></value><value name=\"STAT\"><shadow type=\"inout_highlow\" id=\"yq!;Q}W.XzG=?WI4rY0)\"><field name=\"BOOL\">HIGH</field></shadow></value><next><block type=\"controls_delay\" id=\"ngKcX,fnP|/yn5/[k$=5\"><field name=\"UNIT\">delay</field><value name=\"DELAY_TIME\"><shadow type=\"math_number\" id=\"8M5(YWGYt?,TZ+kW|iv?\"><field name=\"NUM\">500</field></shadow></value></block></next></block></next></block></next></block></statement></block></xml>