<xml version=\"1.2.5\" board=\"Arduino/Genuino Uno\" xmlns=\"http://www.w3.org/1999/xhtml\"><block type=\"base_setup\" id=\"KocBX4Njdo`R:)J+?7QA\" x=\"-236\" y=\"20\"><statement name=\"DO\"><block type=\"serial_begin\" id=\"X^~R8%O;7:X_6pe+%%b@\"><field name=\"serial_select\">Serial</field><value name=\"CONTENT\"><shadow type=\"math_number\" id=\"8cIRKs~7=]bCIx]Rae^|\"><field name=\"NUM\">9600</field></shadow></value></block></statement></block><block type=\"serial_print\" id=\"GcLV3m~gLrZGa.9;4AE8\" x=\"-235\" y=\"104\"><field name=\"serial_select\">Serial</field><field name=\"new_line\">print</field><value name=\"CONTENT\"><block type=\"text\" id=\"=e8-[QLPoY8W|;hl/A:Y\"><field name=\"TEXT\">distance:</field></block></value><next><block type=\"serial_print\" id=\"fgoZT+GL+vgAo?8?JIC~\"><field name=\"serial_select\">Serial</field><field name=\"new_line\">print</field><value name=\"CONTENT\"><block type=\"ks4wd_sr04\" id=\";ws+}{t{HwYxW@iLC(=b\"></block></value><next><block type=\"serial_print\" id=\"y(G{M:j(D2johDFxD!/V\"><field name=\"serial_select\">Serial</field><field name=\"new_line\">println</field><value name=\"CONTENT\"><block type=\"text\" id=\"iBY0w-s@c*r?Xi2$WMHb\"><field name=\"TEXT\">cm</field></block></value><next><block type=\"controls_delay\" id=\".hJnzn7!utndhTwnnKR[\"><field name=\"UNIT\">delay</field><value name=\"DELAY_TIME\"><shadow type=\"math_number\" id=\"2Ulp2jGwnVK1gj!lDxa2\"><field name=\"NUM\">100</field></shadow></value></block></next></block></next></block></next></block></xml>