<xml version=\"1.2.5\" board=\"Arduino/Genuino Uno\" xmlns=\"http://www.w3.org/1999/xhtml\"><block type=\"Mecanum_led\" id=\"zK*$Cx%Jj%-:;@+7q5u7\" x=\"157\" y=\"159\"><field name=\"ledstat\">left_led</field><field name=\"stat\">(1)</field><next><block type=\"Mecanum_led\" id=\"M(zz)T-p-8k`2`r{q?e?\"><field name=\"ledstat\">right_led</field><field name=\"stat\">(1)</field><next><block type=\"controls_delay\" id=\"/^LA^N~^lPa*W;=}!S_Q\"><field name=\"UNIT\">delay</field><value name=\"DELAY_TIME\"><shadow type=\"math_number\" id=\"},%P5:$p3%r7kkNVP,JK\"><field name=\"NUM\">3000</field></shadow></value><next><block type=\"Mecanum_led\" id=\"MfGTLYleWCT|GxKo@nki\"><field name=\"ledstat\">left_led</field><field name=\"stat\">(0)</field><next><block type=\"Mecanum_led\" id=\"c/%f,O=],zBov-nvzx|%\"><field name=\"ledstat\">right_led</field><field name=\"stat\">(0)</field><next><block type=\"controls_delay\" id=\"8(wakLW0St3FIM$.NQrf\"><field name=\"UNIT\">delay</field><value name=\"DELAY_TIME\"><shadow type=\"math_number\" id=\"(IN$pZ+FAd[)ho$,a:M4\"><field name=\"NUM\">1000</field></shadow></value></block></next></block></next></block></next></block></next></block></next></block></xml>