<xml version=\"1.2.5\" board=\"Arduino/Genuino Uno\" xmlns=\"http://www.w3.org/1999/xhtml\"><block type=\"base_setup\" id=\"wX$L_!,jxMCNw2NG;zFj\" x=\"-434\" y=\"-112\"><statement name=\"DO\"><block type=\"serial_begin\" id=\"X^~R8%O;7:X_6pe+%%b@\"><field name=\"serial_select\">Serial</field><value name=\"CONTENT\"><shadow type=\"math_number\" id=\"8cIRKs~7=]bCIx]Rae^|\"><field name=\"NUM\">9600</field></shadow></value></block></statement></block><block type=\"ks4wd_bluetooth\" id=\"?6FHV2nYm-8MpYYyGM4}\" x=\"-437\" y=\"-26\"><field name=\"VAL\">bluetooth_val</field><statement name=\"DO\"><block type=\"serial_print\" id=\"aW~npRE7kDul]-joR0F{\"><field name=\"serial_select\">Serial</field><field name=\"new_line\">println</field><value name=\"CONTENT\"><block type=\"variables_get\" id=\"7nEkmdIrc--LWk/CZ5H^\"><field name=\"VAR\">bluetooth_val</field></block></value></block></statement><next><block type=\"controls_delay\" id=\"+)p.}$De%]RzSV|JGZqR\"><field name=\"UNIT\">delay</field><value name=\"DELAY_TIME\"><shadow type=\"math_number\" id=\"mJ`EYM6.87q-!].d0tSY\"><field name=\"NUM\">200</field></shadow></value></block></next></block></xml>