# Adafruit TCS34725 Color Sensor Driver[![Build Status](https://github.com/adafruit/Adafruit_TCS34725/workflows/Arduino%20Library%20CI/badge.svg)](https://github.com/adafruit/Adafruit_TCS34725/actions)[![Documentation](https://github.com/adafruit/ci-arduino/blob/master/assets/doxygen_badge.svg)](http://adafruit.github.io/Adafruit_TCS34725/html/index.html)

<a href="https://www.adafruit.com/product/1334"><img src="assets/board.jpg?raw=true" width="500px"></a>

This driver is for the Adafruit TCS34725 Breakout.

Tested and works great with the Adafruit MCP9808 Breakout Board 
* http://www.adafruit.com/products/1334

These modules use I2C to communicate, 2 pins are required to  
interface

Adafruit invests time and resources providing this open source code, 
please support Adafruit and open-source hardware by purchasing 
products from Adafruit!

Written by Kevin (KTOWN) Townsend for Adafruit Industries.
BSD license, check license.txt for more information
All text above must be included in any redistribution

To install, use the Arduino Library Manager and search for 'Adafruit TCS34725' and install the library
